8: kd> !sysinfo smbios
[SMBIOS Data Tables v3.2]
[DMI Version - 0]
[2.0 Calling Convention - No]
[Table Size - 4585 bytes]

[BIOS Information (Type 0) - Length 26 - Handle 0000h]
  Vendor                        American Megatrends Inc.
  BIOS Version                  FB01
  BIOS Starting Address Segment f000
  BIOS Release Date             06/20/2019
  BIOS ROM Size                 1000000
  BIOS Characteristics
       07: - PCI Supported
       11: - Upgradeable FLASH BIOS
       12: - BIOS Shadowing Supported
       15: - CD-Boot Supported
       16: - Selectable Boot Supported
       17: - BIOS ROM Socketed
       19: - EDD Supported
       23: - 1.2MB Floppy Supported
       24: - 720KB Floppy Supported
       25: - 2.88MB Floppy Supported
       26: - Print Screen Device Supported
       27: - Keyboard Services Supported
       28: - Serial Services Supported
       29: - Printer Services Supported
       32: - BIOS Vendor Reserved
  BIOS Characteristic Extensions
       00: - ACPI Supported
       01: - USB Legacy Supported
       08: - BIOS Boot Specification Supported
       10: - Enable Targeted Content Distribution
       11: - UEFI Specification Supported
  BIOS Major Revision           5
  BIOS Minor Revision           13
  EC Firmware Major Revision    3
  EC Firmware Minor Revision    1
  Extended BIOS ROM Size        16 MB
[System Information (Type 1) - Length 27 - Handle 0001h]
  Manufacturer                  GIGABYTE
  Product Name                  AERO 17-SA
  Version                       Default string
  Serial Number                 SN19350J000873
  UUID                          00000000-0000-0000-0000-000000000000
  Wakeup Type                   Power Switch
  SKUNumber                     P77SA
  Family                        AERO
[BaseBoard Information (Type 2) - Length 15 - Handle 0002h]
  Manufacturer                  GIGABYTE
  Product                       AERO 17-SA
  Version                       Default string
  Serial Number                 Default string
  Asset Tag                                   
  Feature Flags                 09h
       00: - Motherboard
       03: - Replaceable
  Location                      Default string
  Chassis Handle                0003h
  Board Type                    0ah - Processor/Memory Module
  Number of Child Handles       0
[System Enclosure (Type 3) - Length 22 - Handle 0003h]
  Manufacturer                  GIGABYTE
  Chassis Type                  Notebook
  Version                       y.y
  Serial Number                               
  Asset Tag Number                            
  Bootup State                  Safe
  Power Supply State            Safe
  Thermal State                 Safe
  Security Status               None
  OEM Defined                   0
  Height                        0U
  Number of Power Cords         1
  Number of Contained Elements  0
  Contained Element Size        3
[Onboard Devices Information (Type 10) - Length 6 - Handle 0021h]
Note: The On Board Device Information (Type 10) struct is obsolete as of SMBIOs spec v2.6  Number of Devices             1
  01: Type                      Video [enabled]
  01: Description                  To Be Filled By O.E.M.
[OEM Strings (Type 11) - Length 5 - Handle 0022h]
  Number of Strings             1
   1                            Default string
[System Configuration Options (Type 12) - Length 5 - Handle 0023h]
[Physical Memory Array (Type 16) - Length 23 - Handle 003ah]
  Location                      03h - SystemBoard/Motherboard
  Use                           03h - System Memory
  Memory Error Correction       03h - None
  Maximum Capacity              67108864KB
  Memory Error Inf Handle       [Not Provided]
  Number of Memory Devices      4
[Memory Array Mapped Address (Type 19) - Length 31 - Handle 003fh]
  Starting Address              00000000h
  Ending Address                00ffffffh
  Memory Array Handle           003ah
  Partition Width               02
  Extended Starting Address     0000000000000000h
  Extended Ending Address       0000000000000000h
[ (Type 256) - Length 31 - Handle 0040h]
[ (Type 256) - Length 26 - Handle 0041h]
[ (Type 256) - Length 26 - Handle 0042h]
[ (Type 256) - Length 82 - Handle 0043h]
[ (Type 256) - Length 54 - Handle 0044h]
[ (Type 256) - Length 12 - Handle 0045h]
[Cache Information (Type 7) - Length 27 - Handle 0046h]
  Socket Designation            L1 Cache
  Cache Configuration           0180h - WBEnabled Int NonSocketed L1
  Maximum Cache Size            0180h - 384K
  Installed Size                0180h - 384K
  Supported SRAM Type           0020h - Synchronous 
  Current SRAM Type             0020h - Synchronous 
  Cache Speed                   0ns
  Error Correction Type         ParitySingle-Bit ECC
  System Cache Type             Unified
  Associativity                 8-way Set-Associative
  Maximum Cache Size 2          180 - 00000384l Kb
  Installed Cache Size 2        180 - 00000384l Kb
[Cache Information (Type 7) - Length 27 - Handle 0047h]
  Socket Designation            L2 Cache
  Cache Configuration           0181h - WBEnabled Int NonSocketed L2
  Maximum Cache Size            0600h - 1536K
  Installed Size                0600h - 1536K
  Supported SRAM Type           0020h - Synchronous 
  Current SRAM Type             0020h - Synchronous 
  Cache Speed                   0ns
  Error Correction Type         Multi-Bit ECC
  System Cache Type             Unified
  Associativity                 4-way Set-Associative
  Maximum Cache Size 2          600 - 00001536l Kb
  Installed Cache Size 2        600 - 00001536l Kb
[Cache Information (Type 7) - Length 27 - Handle 0048h]
  Socket Designation            L3 Cache
  Cache Configuration           0182h - WBEnabled Int NonSocketed L3
  Maximum Cache Size            3000h - 12288K
  Installed Size                3000h - 12288K
  Supported SRAM Type           0020h - Synchronous 
  Current SRAM Type             0020h - Synchronous 
  Cache Speed                   0ns
  Error Correction Type         Specification Reserved
  System Cache Type             Unified
  Associativity                 16-way Set-Associative
  Maximum Cache Size 2          3000 - 00012288l Kb
  Installed Cache Size 2        3000 - 00012288l Kb
[Processor Information (Type 4) - Length 48 - Handle 0049h]
  Socket Designation            U3E1
  Processor Type                Central Processor
  Processor Family              c6h - Intel Pentium M processor
  Processor Manufacturer        Intel(R) Corporation
  Processor ID                   ea060900fffbebbf
  Processor Version             Intel(R) Core(TM) i7-9750H CPU @ 2.60GHz
  Processor Voltage             89h - 0.9V
  External Clock                100MHz
  Max Speed                     8300MHz
  Current Speed                 2475MHz
  Status                        Enabled Populated
  Processor Upgrade             Socket BGA1440
  L1 Cache Handle               0046h
  L2 Cache Handle               0047h
  L3 Cache Handle               0048h
  Serial Number                                       
  Asset Tag Number                                    
  Part Number                   To Be Filled By O.E.M.
  Core Count                    6
  Core Enabled                  6
  Thread Count                  12
  Processor Characteristics     fc
  Enabled Characteristics: 
       0x 2: 64-bit Capable
       0x 3: Multi-Core
       0x 4: Hardware Thread
       0x 5: Execute Protection
       0x 6: Enhanced Virtualization
       0x 7: Power/Performance Control
  Processor Family 2            00c6h - Intel Pentium M processor
  Core Count 2                  6
  Core Enabled 2                6
  Thread Count 2                12
[Memory Device (Type 17) - Length 84 - Handle 004ah]
  Memory Error Info Handle      [Not Provided]
  Total Width                   64 bits
  Data Width                    64 bits
  Size                          8192MB
  Form Factor                   0dh - SODIMM
  Device Set                    [None]
  Device Locator                ChannelA-DIMM0
  Bank Locator                  BANK 0
  Memory Type                   1ah - DDR4
  Type Detail                   0080h - Synchronous
  Speed                         3200MHz
  Manufacturer                  Micron
  Serial Number                         
  Asset Tag Number                        
  Part Number                   8ATF1G64HZ-3G2J1    
  Attributes                    1
  Extended Size                 0
  Configured Memory Speed       2667
  Minimum Voltage               1200
  Maximum Voltage               1200
  Configured Voltage            1200
  Memory Technology             3
  Memory Operating Mode Capability     8
  Firmware Version              0
  Module Manufacturer Id        11264
  Module Product Id             0
  Memory Subsystem Controller Manufacturer Id  0
  Memory Subsystem Controller Product Id       0
  Non-Volatile Size             0
  Volatile Size                 0
  Cache Size                    0
  Logical Size                  0
[Memory Device (Type 17) - Length 84 - Handle 004bh]
  Memory Error Info Handle      [Not Provided]
  Total Width                   0 bits
  Data Width                    0 bits
  Size                          [Not Populated]
  Form Factor                   02h - Unknown
  Device Set                    [None]
  Device Locator                ChannelA-DIMM1
  Bank Locator                  BANK 1
  Memory Type                   02h - Unknown
  Type Detail                   0000h -
  Speed                         0MHz
  Manufacturer                  [String Not Specified]
  Serial Number                 [String Not Specified]
  Asset Tag Number              [String Not Specified]
  Part Number                   [String Not Specified]
  Attributes                    0
  Extended Size                 0
  Configured Memory Speed       0
  Minimum Voltage               0
  Maximum Voltage               0
  Configured Voltage            0
  Memory Technology             0
  Memory Operating Mode Capability     0
  Firmware Version              0
  Module Manufacturer Id        0
  Module Product Id             0
  Memory Subsystem Controller Manufacturer Id  0
  Memory Subsystem Controller Product Id       0
  Non-Volatile Size             0
  Volatile Size                 0
  Cache Size                    0
  Logical Size                  0
[Memory Device (Type 17) - Length 84 - Handle 004ch]
  Memory Error Info Handle      [Not Provided]
  Total Width                   64 bits
  Data Width                    64 bits
  Size                          8192MB
  Form Factor                   0dh - SODIMM
  Device Set                    [None]
  Device Locator                ChannelB-DIMM0
  Bank Locator                  BANK 2
  Memory Type                   1ah - DDR4
  Type Detail                   0080h - Synchronous
  Speed                         3200MHz
  Manufacturer                  Micron
  Serial Number                         
  Asset Tag Number                        
  Part Number                   8ATF1G64HZ-3G2J1    
  Attributes                    1
  Extended Size                 0
  Configured Memory Speed       2667
  Minimum Voltage               1200
  Maximum Voltage               1200
  Configured Voltage            1200
  Memory Technology             3
  Memory Operating Mode Capability     8
  Firmware Version              0
  Module Manufacturer Id        11264
  Module Product Id             0
  Memory Subsystem Controller Manufacturer Id  0
  Memory Subsystem Controller Product Id       0
  Non-Volatile Size             0
  Volatile Size                 0
  Cache Size                    0
  Logical Size                  0
[Memory Device (Type 17) - Length 84 - Handle 004dh]
  Memory Error Info Handle      [Not Provided]
  Total Width                   0 bits
  Data Width                    0 bits
  Size                          [Not Populated]
  Form Factor                   02h - Unknown
  Device Set                    [None]
  Device Locator                ChannelB-DIMM1
  Bank Locator                  BANK 3
  Memory Type                   02h - Unknown
  Type Detail                   0000h -
  Speed                         0MHz
  Manufacturer                  [String Not Specified]
  Serial Number                 [String Not Specified]
  Asset Tag Number              [String Not Specified]
  Part Number                   [String Not Specified]
  Attributes                    0
  Extended Size                 0
  Configured Memory Speed       0
  Minimum Voltage               0
  Maximum Voltage               0
  Configured Voltage            0
  Memory Technology             0
  Memory Operating Mode Capability     0
  Firmware Version              0
  Module Manufacturer Id        0
  Module Product Id             0
  Memory Subsystem Controller Manufacturer Id  0
  Memory Subsystem Controller Product Id       0
  Non-Volatile Size             0
  Volatile Size                 0
  Cache Size                    0
  Logical Size                  0
[Memory Device Mapped Address (Type 20) - Length 35 - Handle 004eh]
  Starting Address              00000000h
  Ending Address                007fffffh
  Memory Device Handle          004ah
  Mem Array Mapped Adr Handle   003fh
  Partition Row Position        [Unknown]
  Extended Starting Address     0000000000000000h
  Extended Ending Address       0000000000000000h
[Memory Device Mapped Address (Type 20) - Length 35 - Handle 004fh]
  Starting Address              00800000h
  Ending Address                00ffffffh
  Memory Device Handle          004ch
  Mem Array Mapped Adr Handle   003fh
  Partition Row Position        [Unknown]
  Extended Starting Address     0000000000000000h
  Extended Ending Address       0000000000000000h
[ (Type 256) - Length 20 - Handle 0050h]
[ (Type 256) - Length 64 - Handle 0051h]
[ (Type 256) - Length 11 - Handle 0057h]
[ (Type 256) - Length 11 - Handle 0058h]
[ (Type 256) - Length 11 - Handle 0059h]
[ (Type 256) - Length 11 - Handle 005ah]
[ (Type 256) - Length 11 - Handle 005bh]
[ (Type 256) - Length 11 - Handle 005ch]
[ (Type 256) - Length 11 - Handle 005dh]
[ (Type 256) - Length 11 - Handle 005eh]
[ (Type 256) - Length 11 - Handle 005fh]
[ (Type 256) - Length 11 - Handle 0060h]
[ (Type 256) - Length 89 - Handle 0061h]
[ (Type 256) - Length 6 - Handle 0062h]
[ (Type 256) - Length 106 - Handle 0065h]
[ (Type 256) - Length 4 - Handle 0066h]
